SOUTH

** this test was conducted with 
0) antenna under test: s/n 4846A60371 (TRM59800.00), 10.0 Sokkia standoff
1) Ashtech chokering on reference pier
2) standard tracking loop settings for 689 PTU rx
      2a) Parameters > Advanced > Multipath Reduction
	for both receivers
	carrier : mpnew
	code : mpnew
	(rx defaults)
3) last rx reset - immediately before test (Javad and Sept)


start of test
7  5 13 0 0 0 
end of test
7  5 13 2 10 6
duration: 2.06  hours

files at start of test
689_0507a
699_0507a
log0000.sbf

files at end of test 
689_0506b leaving off last 10 minutes
699_0506b
log0001.sbf


(standard):
  /par/raw/gdplls={band=3.0,order=1,guid=100}
  /par/raw/plls={band=3.0,order=1,guid=100}
