SOUTH

previous south tests are giving 1-d results which deviate
from all other directions.  Rerunning to confirm.

** this test was conducted with 
0) antenna under test: s/n 4846A60371 (TRM59800.00), 10.0 Sokkia standoff
1) Ashtech chokering on reference pier
2) standard tracking loop settings for 689 PTU rx
      2a) Parameters > Advanced > Multipath Reduction
	for both receivers
	carrier : mpnew
	code : mpnew
	(rx defaults)
3) last rx reset - 2 days ago


start of test
8  5 13 21 4 13
end of test
8  5 13 23 14 25
duration: 2.00 hours

files at start of test
689_0508v
699_0508v
log0000.sbf

files at end of test 
689_0508x
699_0508x
log0001.sbf


(standard):
  /par/raw/gdplls={band=3.0,order=1,guid=100}
  /par/raw/plls={band=3.0,order=1,guid=100}
