start of test
26  3  13 17 55 23
end of test
26  3  13 20 4 41
duration: 1.99 hours

files at start of test
689_0326s (at start of motions)
699_0326s
C:\Documents and Settings\AntCal\My Documents\AsteRx\log_0000.sbf

files at end of test
689_0326u
699_0326u
C:\Documents and Settings\AntCal\My Documents\AsteRx\log_0001.sbf


** this test was conducted with 
0) ITT chokering (sn 109) + SCIS dome
1) Ashtech chokering on reference pier
2) standard tracking loop settings for 689 PTU rx



(standard):
  /par/raw/gdplls={band=3.0,order=1,guid=100}
  /par/raw/plls={band=3.0,order=1,guid=100}
